Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

© 1999 IEEE. Personal use of this material is permitted. However, permission to reprint/republish this

material for advertising or promotional purposes or for creating new collective works for resale or

redistribution to servers or lists, or to reuse any copyrighted component of this work in other works must be

obtained from the IEEE.

ABSTRACT

A very important problem in fade countermeasure systems is the need to detect signal quality

quickly and accurately. In fact, the countermeasure has to be initiated before the signal degradation

effect on the bit error rate is detected by the user. This paper presents an overview of different

methods to evaluate signal quality, which are based on the availability of soft quantized levels of

PSK demodulated signals at the receiver. It is shown that this class of methods has a good

theoretical performance. Also, an innovative procedure is presented which adapts one of the

methods to some existing hardware, and tunes-up a set of parameters in order to compensate to the

fact that the hardware is to some extent impaired.

__________________

                                                                                                        QUAL

                                                                                                    IT

                                                                                                   Y

                                                                                                EST

                                                                                                IMAT

                                                                                             ION OF  PSK

                                                                                                MODUL

                                                                                              AT

                                                                                          ED SIGNAL

                                                                                            S

Nedo Celandroni

N.Celandroni@cnuce.cnr.it

Erina Ferro E.Ferro@cnuce.cnr.it

Francesco Potortì

F.Potorti@cnuce.cnr.it

CNUCE, Institute of National Research Council

Via S. Maria 36 - 56126 Pisa - Italy

Phone: +39-50-593111 (operator); Fax: +39-50-904052; Telex: 500371

T

                                he use of the Ka band (30/20 GHz) for satellite communication systems raises the problem of

dealing with rain attenuation. As opposed to the traditionally used Ku band (14/12 GHz), the Ka

band is much more affected by atmospheric events that lead to bad signal conditions, ranging from

a slowly changing attenuation of the signal to a sudden deep fade that blocks all communication.

Many methods for countermeasuring rain attenuation have been proposed [1-9]. Some of these

methods, such as space or frequency diversity [7, 9], allow a very high level of link availability to

be achieved, but they are very complex and expensive. Other methods, which are based on the

dynamic adjustment of the energy per information bit [1-3], can be employed when a moderate

level of link availability is required. They are not very complex and are cost effective. These

methods require a modem that is able to change the transmitting power and the data bit rates, and a

convolutional encoder/Viterbi decoder with puncturing, in order to realize a real variable coding

rate.

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

All fade countermeasure systems require an attenuation meter that can make accurate estimates of

signal degradation in real time, in order to trigger the countermeasure in a timely fashion. When the

transmission power control is used to compensate for up-link attenuation, the latter must be

estimated separately from the down-link attenuation. A traditional method of measuring the signal

attenuation is to use beacon receivers at the earth stations. This requires beacon transmitters at

frequencies that are very close to the signal frequency bands. Two beacon transmitters at the

satellite and two receivers at each earth station are necessary if one needs to distinguish between

the attenuations on the up- and down-links. The big drawback of this method is the high cost of the

hardware required. The other disadvantage is that the measurement of the attenuation is made out

of signal band, and this leads to inaccuracies. In fact, even if the beacon and the signal frequencies

are very close together, there is always some uncorrelation between the relative attenuation values.

Another method to estimate attenuation is by measuring the power level of the received signal

which, given a clear-sky reference level, depends on the up- and down-link attenuations. For a

digital modem, this usually requires little additional hardware, because the modem already needs

an instantaneous measure of the power level received, which is made with a fast AGC (automatic

gain control) in order to demodulate the data. This method is very cheap and does not lead to

inaccuracies due to the measurement frequency offset, but it does not allow a separate evaluation of

the up- and down-link attenuations.

An alternative way to estimate signal quality is to evaluate the signal to noise ratio (SNR), from

which an evaluation of the bit error rate (BER) is straightforward. This method is much more

accurate than the signal attenuation measurement, since it takes into account the noise level

variation due to the attenuation, i.e. the changes in sky temperature. Furthermore, SNR evaluation

methods consider the effect of the total noise, including interference. Not even by using this

method the contributes of the up- and down-link attenuations can be distinguished.

The SNR evaluation methods referred to in this paper deal with considering the power distribution

of the received signal around its mean value. In the following we show how this measure can be

made with very little additional hardware, provided that the receiver is equipped with a soft

decision level convolutional decoder. With respect to measuring the received power level, this

method has the additional advantage of being independent of any reference level, thus requiring no

tuning by an operator. It can thus be useful for end-user equipment, such as mobile, nomadic, or

hand-held terminals, where ease of use is an essential requirement.

In the following, a set of methods to estimate the E

b

/ N

0

 ratio, in an additive white Gaussian noise

environment, are presented in order of increasing performance and complexity.

CHANNEL QUALITY ESTIMATION USING BER

Methods of measuring the signal quality that do not rely on dedicated (beacon) receivers have to

rely on the characteristics of the received signal itself. In optimal coherent detection of B/QPSK

(binary/quadrature phase-shift-keyed) signals, the BER is a function of the channel E

b

/ N

0

[22]

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

BER

=

1

2
erfc  (
r
) ,  where   erfc x

( )

=

D

2

p
e

-
t

2

x

¥

ò

dt    and
r =

D

E

b

/ N

0

. (1)

The instantaneous E

b

/ N

0

 can thus be computed by directly measuring the BER of the signal

before the convolutional decoder at the receiver. This is done by re-encoding the decoded data and

comparing the resulting bit stream with the input bit stream, as shown in Fig. 1.

demodulator
soft quantizer

Viterbi decoder
received

data

delay

convolutional

encoder
error counter

signal quality

F igure 1.  Block diagram of BER counter.

Only the errors recovered by the convolutional decoder are counted, but the approximation is

generally very good. For example, from Fig. 2 we can deduce that for E

b

/ N

0

 values greater than

0  dB, less than 1% of the bit errors are undetected, and less than 0.1% for E

b

/ N

0

 greater than

1  dB. This method is simple, but it has very low precision (or alternatively it is very slow) at high

E

b

/ N

0

 values.  The probability of detecting n  errors by inspecting N   bits is

P

n

=

N

n
æ

è
ç
ö

ø

 p

e
n
1

-

p

e

( )

N

-
n

. (2)

0

5000

10000

15000

20000

25000

30000

Number of bits

1E-06

1E-05

0.0001

0.001

0.01

0.1

BER

0 1 2 3 4 5 6 7

Channel  Eb/No [dB]

1/2 coded data BER

Uncoded data BER

Nunber of bits

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

F igure 2.  Number of bits needed to evaluate Eb/No using BER.  1/2

coded data BER as a function of  the channel Eb/No, and uncoded data

BER are also reported.

The above binomial distribution has μ  =  n / N , and variance
s 2 =

p

e

( 1

-

p

e

) / N  [21]. When the

product Np

e

 is large, which is always the case for any significant measure of this kind, we can

approximate the binomial distribution with a Gaussian distribution that has the same mean and

variance. Denoting by R  the
E

b

/ N

0

 expressed in dB, that is R  =  10  log

10

(
E

b

/ N

0

), the estimated

value of R  can be obtained by inverting the monotonic function (1). When the variance of the

estimator p

e

 is small, the distribution of the estimate of R  can be considered Gaussian as well, with

mean and variance

                                                                                                             m

R

=
R p

e

( )

,
s

R

2 =
p

e

 ( 1

-
p

e

)

dp

e

R

( )

/ dR

( )
2

N

. (3)

A measure of the precision of the method is thus given by the number N  of symbols that must be

examined to get a measure with a 99% confidence interval of ±0.5  dB, which is

                                                                                                                N

=

2 . 58 2
s

R

2

0 . 5

2

,  since  erfc

2 . 58

2
æ

è
ö

ø

=
1 % . (4)

However, the variance of the estimator p

e

 is not always small, so the distribution of the estimate of

R  is not Gaussian, and using (4) may lead to an optimistic evaluation of N . However we can use (4)

if, instead of (3), we adopt an overestimation of the variance given by

                                                                                                             s

R

2 =
p

e

( 1

-
p

e

)

D
p

e

R

( )

/

D
R

( )
2

N

 ,    (5)

where

                                                                                                            D
p

e

/

D
R

=
min

D
p

e

/

D
R

[ ]
+

,

D
p

e

/

D
R

[ ]
-

{ }

,  [·]

+
 and [·]

-
 are the right and left incremental

ratios, respectively, and

D
R

=
2 . 58
s

R

. The resulting N   obtained with this method is plotted in

Fig. 2.

CHANNEL QUALITY ESTIMATION USING PSEUDO ERRORS

In [10] a variety of methods for measuring the signal attenuation are summarized. In particular, a

technique is described which implies measuring the PSK  signal amplitude vector and estimating its

variance. A simple variation on this theme, described in [11, 16], is valid for B/QPSK. This

variation can be inexpensively applied to all coherent demodulators that produce a soft-level

quantization of demodulated data for a convolutional (typically Viterbi) decoder.

demodulator
soft quantizer

Viterbi decoder
received

data

n

weighted

accumulator
signal

quality

F igure 3.  Block diagram of the quality meter.

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

Figure 3 shows a block diagram of the arrangement, which only requires a small finite state

machine connected to the output of the soft quantizer. The method we are going to describe, as well

as all the following ones, applies to both BPSK and QPSK modulated signals, since QPSK can be

considered as two independent (in-phase and quadrature) channels.

It is easy to count the number of times the demodulated quantized signal S  falls below a designated

threshold T
m

s

, where
m

s

 is the expected value of S  and 0< T <1, and then to obtain the frequency of

such an event ( pseudo error ). Figure 4 depicts this concept.

7 6 5 4 3 2 1 0

0 T
m

s
m

s

F igure 4.  The quantized signal when T=5/8

The probability of the signal S  being smaller than T
m

s

, i.e. the probability of a pseudo error, is

given by

                                                                                                                 P S

<
T
m

s

{ }

=

1

2
erf 2 1

-
T

( )

r
,  1

+
T

( )

r

( )

,  where
erf 2 a , b

( )

=

D

2

p

 e

-
t

2

a
b

ò

dt

. (6)

Only the magnitude of the signal is considered, without any knowledge of whether the bit has been

correctly decoded. Function (6) can be inverted, so the
E

b

/ N

0

 and the BER of the signal can be

obtained from the frequency of the event
S

<

T
m

s

{ }

. This method can be analyzed analogously to

the measure of the BER presented in the previous section using (6) instead of (1).   The results are

plotted in Fig. 5 for different values of the threshold T . We can see that a good performance can be

obtained by choosing the value of T  that gives the maximum sensitivity in the range of interest of

the application. The drawbacks of this method are the limited size of the application field for each

value of the threshold, and the bad performance at very low
E

b

/ N

0

 values. In this last case the

BER method performs much better, as shown in Fig. 5.

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

3000

4000

5000

6000

7000

8000

9000

10000

11000

12000

Number of bits

0 2 4 6 8 10 12 14 16 18 20 22

Eb/No [dB]

T=7/8

T=6/8

T=5/8

T=4/8

T=3/8

T=2/8

T=1/8

BER

F igure 5.  Number of bits needed to evaluate Eb/No using the pseudo

error method.

IMPROVED CHANNEL QUALITY ESTIMATION SYSTEMS

An improvement to the pseudo error method has been proposed in [12]. Figure 4 highlights that a

lot of information is thrown away when the pseudo error method is used. Indeed, for each symbol,

the measure of the amplitude, which is an n  bit quantity, is used to find out whether or not the

symbol amplitude is below the threshold, which is a one bit information. On the other hand, if we

use the average discrete amplitude of the signal, we manage to use much more information. We

call this the method of the mean .

We assume that the region between 0 and μ

s

 is divided (quantized) into q  equal-sized regions,

numbered from 0 to q -1, and that when the signal exceeds μ

s

 it is considered as belonging to the

region labelled with "0". This is the way the signal in input to a Viterbi decoder is usually

quantized, although in [18] it is argued that some improvements can be obtained by slightly

changing the quantization step. The mathematical analysis of this method follows the same

guidelines as the previous methods, but instead of (1) used in the BER method or (6) used in the

pseudo error method, we use (7), which is invertible as well.

M
r

( )

=

1

2
i erf 2
i

q
r

,
i

+

1

q
r
æ

è
ç
ö

ø

+

erf 2 2

-
i

+

1

q
æ

è
ç
ö

ø
r

, 2

-
i

q
æ

è
ç
ö

ø
r
æ

è
ç
ö

ø

÷
é

ë
ê
ù

û
ú

i = 1
q - 1

å

. (7)

Relation (7) assumes that the magnitude of a bit is measured, regardless of whether the bit has been

correctly received or not. By using a logic similar to the one shown in Fig. 1, it is possible to know,

for each bit, whether or not it has been correctly received. This additional information can be used

to improve the performance of the quality meter. In this case, instead of (7), we have:

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

M

e
r

( )

=

1

2
i erf 2
i

q
r
,
i

+
1

q
r
æ

è
ç
ö

ø

i

=
1

2 q

-
2

å

+

1

2

2 q

-
1

( )

erfc 2

-

1

q
æ

è
ç
ö

ø
r
æ

è
ç
ö

ø

÷

.

In [12,13] it is shown that the choice of q =8 is a good compromise between performance and

complexity, so this value is assumed throughout the rest of the paper. The performance of this

method is shown in Fig. 6, with and without the use of the error bit logic.

0

1000

2000

3000

4000

5000

6000

7000

8000

Number of bits

0 2 4 6 8 10 12 14 16 18 20 22

Eb/No [dB]

 with error bit

 without error bit
with error bit
without error bit
normal quantization
extended

 quantization

q = 8

F igure 6. Number of bits needed to evaluate E

b

/ N

0

 using the method of the mean.

7 6 5 4 3 2 1 0

0
m

s

F igure 7. Extended quantization, assuming n = 3.

In [13] another improvement is proposed to the method of the mean, which the authors call

extended quantization . This method requires a modification to the quantization logic, as shown in

Fig. 7, and the block diagram shown in Fig. 3 does not hold any more, because some little logic

must be added to the quantizer, in order to obtain both the outputs for the Viterbi decoder and the

extended quantization meter.

As shown in Fig. 6, the precision achieved by this method is considerably better than the normal

quantization  method, because about twice the information is gathered.

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

REFINEMENTS TO THE METHOD OF THE MEAN

The demand assignment FODA/IBEA TDMA
1

 access scheme [2, 3], developed in the framework

of experimental projects on the Olympus satellite, requires a signal quality measurement in order to

counter the signal fade by using data redundancy.

Indeed, during a signal fade event, data is made redundant (by reducing coding and bit rates) by a

factor that is sufficient to meet some given specifications, typically in the form of a BER threshold.

If the uncertainty on the measure of the fade is large, a proportionally large security margin must

be added to the measured value, in order to guarantee the quality of service desired. This, in turn,

entails increasing the data redundancy, and thus the bandwidth occupied, with a consequent

reduction in the overall utilization efficiency of the channel. The speed of the meter is important as

well. In fact, since the signal fade may have a very fast variation in time, a further uncertainty is

introduced, which increases with the measurement time span. Moreover, since data is received after

the fade is measured, both these margins must be suitably increased because a prediction on the

fading has to be made by the receiver when it informs the transmitter about its own fade situation.

FODA/IBEA was implemented and tested using a prototype modem [4] with an 8 level soft

quantizer of the signal amplitude, followed by a Viterbi decoder. Due the structure of the hardware,

it was impossible to use either the extended quantization or the error bit method, so we used the

normal quantization method without error bit. Given the high bit rate used (8 Mbit/s), we

nonetheless expected a good quickness, but our measures showed a performance much worse than

the theoretical one. This was due to the fact that the reference level, computed by the logic of the

modem, was not stable. In fact, it oscillates with a frequency lower than the symbol rate, thus

invalidating the hypothesis on which the analyses made in the previous section are based. In order

to examine the new situation, we tried to model the behaviour of the modem by superimposing a

sinusoidal wave to the symbol amplitude, thus obtaining a distribution of the amplitude that

deviates from the Gaussian. We obtained a model that matches our measures well, as shown in Fig.

8. In order to deal with such an impaired situation we further refined the method presented in [12].

We thus obtained a procedure which can be ^customized~ to match the particular oddities of a

given modem, and which is guaranteed to get the best possible performance from the hardware for

a given number of quantization levels. This procedure also gives a marginally better performance

in the theoretical case, with respect to the methods presented in the previous section.

In order to maximize the information obtained from the quantized levels, each level is given a

different weight, obtained by numerically minimizing the number of bits needed to get a reliable

measure at the desired values of
E

b

/ N

0

. The methods presented in [11], [12] and [13] are

particular cases of this technique. For example, given a 3 bit (8 level) quantization, the pseudo error

method with T =3 is equivalent to have weights set to 0 0 0 1 1 1 1 1

[ ]

, the method of the

1
            Fifo Ordered Demand Assignment/Information Bit Energy Adaptive - Time Division Multiple Access

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997
mean with normal quantization is equivalent to have a weight vector set to

               0 1 2 3 4 5 6 7

[ ]

, and the method of the mean with extended quantization is equivalent

to have a weight vector set to 3 2 1 0 0 1 2 3

[ ]

. The variance of the measure is invariant

to scaling and translation of the weight vector, which means that using a vector w is equivalent to

using a vector a

+
b w . This implies that the first element of the weight vector can be arbitrarily set

to 0 and the next non-zero element can be set to 1. The optimization thus only needs to be carried

on the remaining elements. When using an arrangement like the one depicted in Fig. 3, the

elements are constrained to be integer (usually small ones). Assuming w 0

[ ]

=
0 , the function we

use is now

                                                                                                             W
r

( )

=

1

2
w
i

[ ]

erf

2
i

q
r

,
i

+
1

q
r
æ

è
ç
ö

ø

+

erf

2 2

-
i

+
1

q
æ

è
ç
ö

ø
r

,

2

-
i

q
æ

è
ç
ö

ø
r
æ

è
ç
ö

ø

÷
é

ë
ê
ù

û
ú

i

=
1
q

-
1

å

. (8)

Whether or not (8) is invertible depends on the weight vector w . However, the minimization of the

variance, which is used to obtain the best value of w , guarantees that (8) is monotonic and thus

invertible. In fact, in the points where (8) has a null derivative an infinite number of bits would be

required to get an estimate. Figure 8 shows the performance of the weighted quantization .

The weight vector used for the real case is 0 1 3 6 10 15 20 27

[ ]

.

If the hardware allows to set the span of the quantization levels, other interesting results can be

obtained. Using normal quantization, the signal levels are set to i
m

s

/ q  where i  =  0,1,2,...q-1, while

using extended quantization the levels are set to 2 i
m

s

/ q . If the hardware allows the levels to be set

to ki

                                                                      m

                                                                                             s

                                                                                                         , where k  is a tuneable quantity, a further improvement can be obtained by appropriately

choosing k  and w.  In practice, our results showed that the optimum k  is very close to the situation

where one of the quantization zones is centred on the Gaussian, that is, when k  =  2/( q -1) (Fig. 9).

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

0.01

0.1

1

10

Mean quality

3000

4000

5000

6000

7000

8000

9000

10000

11000

Number of bits

2 4 6 8 10 12 14 16 18 20

Eb/No [dB]
mdl nb linear weights
mdl nb opt weights

th  nb opt weights
th nb linear weights
ms nb opt weights
th ql opt weights
mdl ql opt weights
ms ql opt weights

th = theoretical

mdl = model

nb = number of bits

ql = mean quality

opt = optimized

ms = measured

F igure 8.  Mean quality and sample size using normal quantization, as functions of

E

b

/ N

0

. Theoretical, modelled and real cases.

7 6 5 4 3 2 1 0

0
m

s

F igure 9.  Optimized extended quantization.

In Fig. 10 the performances of extended quantization are shown, both with linear weights (method

of the mean) and with optimized levels and weights. The improvement due to the adoption of the

error bit is shown as well.

We have shown that the methods outlined in this paper for measuring the
E

b

/ N

0

 ratio of a

BPSK/QPSK signal by using soft level quantization improve on each other. There is a limit to this

improvement, which is plotted in Fig. 10 as a horizontal line that indicates the minimum possible

number of bits needed to get the required precision, assuming that the signal amplitude can be

measured with an arbitrary precision. In order to obtain this result, let us consider that measuring

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997
the amplitude of N  demodulated bits is equivalent to taking N  samples from a normal distribution.

We are interested in the variance of this distribution, that is, the N

o

 value, given that E

b

 is

normalized to 1. The error we make in measuring the variance can be evaluated by considering the

distribution of the measure of the variance, and using it to obtain a confidence interval for the

measured variance. Thus we can say that we are taking N  samples z

i

 with a normal distribution

N
m
,
s 2

( )

, and we estimate the sample variance as

�
s

2
=

1

N
z

i

- m

( )

2

1

N

å

. The random variable

N

�
s 2
/
s 2
 follows a
c

2
N

( )

 distribution [19] which, for N  >100, is well approximated by

N N ,  2 N

( )

 [20]. In order to match the 99% confidence interval of ±0.5 dB that we have used

throughout this article, we consider a 99% confidence interval of 10

-
0 . 5 / 10

,

10

+
0 . 5 / 10

[ ]

 computed on

the
c

2
N

( )

/ N  distribution. Such an interval is asymmetric. Instead of this, for simplicity we use

the symmetric conservative interval

±
1

-
10

-
0 . 5 / 10

( )

. The optimum number of bits
N

opt

 can thus be

computed by using the relation 2
.

58 2
/ N

opt

=
1

-
10

-
0 . 5 / 10
.

In [13] the same limit is obtained by assuming an infinite number of quantization levels.

0

1000

2000

3000

4000

5000

Number of bits

0 2 4 6 8 10 12 14 16 18 20 22

Eb/No [dB]
optimum
optimized weigths and levels
linear weights

without error bit

with error bit

F igure 10. Performance of extended quantization. Linear weights and optimized levels and

weights, with and without the error bit logic.

CONCLUSIONS

As the exploitation of the K

a

 band for satellite communication increases, the need for a quick and

accurate estimate of the E

b

/ N

0

 ratio available at the receiver is gaining importance. Since

redundancy-based counterfade systems can be employed even in low-cost implementations, hand-

held appliances can benefit from simple and efficient E

b

/ N

0

 measurement systems. We have

presented (in increasing sophistication and chronological order) a class of methods for evaluating

in real time the E

b

/ N

0

 ratio of a received BPSK/QPSK signal. Apart from the BER method, which

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997
is applicable for very low E

b

/ N

0

 ratios only, we have shown that the theoretical performance of

all the other methods is satisfactory. In particular, the performance of the most sophisticated system

is very close to the best possible attainable performance. All the systems presented are however

very cheap, because they mostly use the logic needed by a Viterbi decoder used in soft quantization

mode, which is the most common technique employed in digital satellite communications. We have

also presented a real case, which uses a novel procedure that optimizes the results, thus limiting the

effects due to the impairments of the realization.

REFERENCES

[1] N. Celandroni, F. Potortì and S. T. Rizzo, ^Signal Quality Monitoring to Counter Rain Fading

                                                                               with Adaptive Information Bit Energy in Satellite Thin Route TDMA Systems~, CNUCE

                                                                               Report C95-44, Dec. 1995.

[2] N. Celandroni, E. Ferro, N. James and F. Potortì, ^FODA/IBEA: a flexible fade

                                                                               countermeasure system in user oriented networks~, Intern. Journal of Satellite

                                                                               Communications, Vol. 10, No. 6, pp. 309-323, 1992.

[3] N. Celandroni, E. Ferro and F. Potortì, ^The performance of the FODA/IBEA satellite access

                                                                               scheme measured on the Italsat satellite~, Proc. of the ICDSC-10 Conference, pp. 332-338,

                                                                               V.1, Brighton 15-19 May 1995.

[4] N. Celandroni, E. Ferro, F. Potortì, A. Bellini and F. Pirri, ^Practical experiences in

                                                                               interconnecting LANs via satellite~, ACG SIGCOMM Computer Communication Review,

                                                                               Vol. 25, No. 5, pp.56-68, October 1995.

[5] M.J. Willis and B.G. Evans, ~Fade countermeasure at Ka band for Olympus^, International

                                                                               Journal of satellite communications, Vol. 6, pp.301-311 1988.

[6] H. Kazama, T. Atsugi, M. Umehira and S. Kato, ^A Feedback-Loop Type Transmission

                                                                               Power Control for Low Speed TDMA Satellite Communication Systems~, Proc. IEEE ICC

                                                                               ´89, Boston MA.

[7] E. Russo, ^Implementation of a space diversity system for Ka-band satellite

                                                                               communications~, IEEE ICC 1993.

[8] L. Dossi, G. Tartara and E. Matricciani, ^Frequency diversity in millimeter wave satellite

                                                                               communications~, IEEE Trans. on Aerospace and Electronic Systems vol. 28, n.2, pp. 567-

                                                                               73, April 1992.

[9] F. Carassa, E. Matricciani and G. Tartara, ^Frequency diversity and its applications~,

                                                                               International Journal of Satellite Communications, vol. 6, pp. 313-322 (1988).

[10] E. G. Randall, ^PSK signal quality estimates for network control~, Milcom `85 - Proceedings

                                                                               of the IEEE Military Communications Conference, October 1985, Boston

[11] N. Celandroni, ^Estimation of the Eb/No ratio using PSK quantized levels in an additive

                                                                               white Gaussian noise (AWGN) environment~, CNUCE Report C90-22, September 1990.

[12] D. Kreuer, E. Bierbaum ^Estimating the signal quality of a digital satellite link using soft

                                                                               quantized bits~, VIII International symposium on Computer and Information science, 1993,

                                                                               Instanbul, Turkey.

[13] D. Kreuer and E.Bierbaum, ^Improved Eb/No Estimation with Soft Quantized Detection~,

                                                                               Proc. PIMRC´94/WCN, Den Haag, The Netherlands, Sept. 1994, pp. 620-624.

[14] CCIR Report 564-4, ^Propagation data and prediction methods required for earth- space

                                                                               telecommunications systems~, 1990.

[15] T.J.Nohara, Al Premji, W.R.Seed, ^A new signal quality degradation monitor for digital

                                                                               transmission channels~, IEEE Trans. on Communications, N. 2/3/4 1995, pp 1333-1336.

Preprint of an article published on the IEEE COMMUNICATIONS  MAGAZINE , July 1997

[16] T. Atsugi et al., "A study on the up-link transmission power control scheme for

                                                                               communication systems", ISAP ’85.

[17] B.K.Lewitt, ^Rain compensation algorithm for ACTS mobile terminal~, IEEE JSAC, vol. 10,

                                                                               No 2, February 1992, pp. 358-363.

[18] Y. Yasuda, X. Hirata, A.Ogawa, "Optimum soft decision for Viterbi decoding", IEEE 5th

                                                                               International Conference on Satellite Communications, Genova, Italy, 1981.

[19] R.V. Hogg, A.T. Craig, "Introduction to mathematical statistics", V Edition, Prentice Hall,

                                                                               1978.

[20] M.C. Jeruchim, P. Balam, K.S. Shanmugam, " Simulation of communication systems", Series

                                                                               Editor: R.W. Lucky, AT&T Bell Laboratories, II Printing, January 1994.

[21] A. Papoulis, "Probability, random variables  and stochastic processes", McGraw-Hill, 1991.

[22] J.G. Proakis, "Digital communications", McGraw-Hill, 1995.